**TEMPOMIX time flow shower mixer**

Single control time flow

Recessed, wall plate Ø 195mm

Reference: **790927**

Specification description

Recessed time flow shower mixer:

Chrome-plated metal wall plate Ø 195mm.

Standard recessing housing.

Recessing depth can be adjusted from 28 - 43mm.

TEMPOMIX ¾" single control mixer.

Ligature-resistant collar.

Temperature control and operation via the push-button.

Maximum temperature limiter (can be adjusted by the installer).

Time flow ~30 seconds.

Flow rate 12 lpm at 3 bar.

M½" connectors for Ø 14mm copper tubes.

Chrome-plated metal control.

Integrated non-return valves and filters.

30-year warranty.

This model does not have a waterproof recessing box. The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).