**TEMPOSTOP time flow shower kit**

Time flow

Exposed, TONIC JET head

Reference: **749001**

Specification description

Exposed time flow shower kit:

TEMPOSTOP time flow valve M¾" for mixed water supply from beneath.

For wall-mounted installation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant TONIC JET shower head with automatic flow rate regulation.

Chrome-plated solid brass.

Reinforced shower column Ø 16mm and collar (mounting bracket and screws supplied).

30-year warranty.