**TEMPOSTOP time flow shower valve**

Time flow

Exposed, with flow rate regulator, M¾"

Reference: **749700**

Specification description

Time flow shower valve for exposed installation:

TEMPOSTOP M¾" time flow valve for in-line mixed water supply.

For wall-mounted exposed installation.

Time flow ~30 seconds.

Flow rate 12 lpm at 3 bar, with flow rate regulator.

Chrome-plated solid brass body and push-button.

30-year warranty.