**TONIC JET shower head**

Scale-resistant

For panel from 1 to 10mm

Reference: **712010**

Specification description

Scale-resistant fixed shower head for panel from 1 to 10mm:

Flow rate 6 lpm at 3 bar.

Automatic flow rate regulation.

Scale-resistant and ligature-resistant nozzle with adjustable spray.

Chrome-plated solid brass.

Fixed with concealed blocking screw.

Systematically drains after use (no water retention or impurity deposits).

Inlets M1/2".

30-year warranty.