**Floor trap**

With plate

140 x 140mm

Reference: **684000**

Specification description

Floor trap for hard floors:

Flow rate 18 lpm.

Water level 18mm.

Stainless steel body 140 x 140mm.

Bright polished stainless steel grid fixed by 1 stainless steel screw.

PVC bell.

Vertical outlet Ø 40mm (provide elbow for horizontal outlets).

For hard floors (tiled or concrete).

30-year warranty.