**TEMPOSOFT 2 time flow urinal valve**

Time flow 3 seconds

Recessed, Soft-touch operation

Reference: **777130**

Specification description

Recessed time flow urinal valve:

For standard or siphon action urinals.

For recessed installation.

Bright polished stainless steel wall plate Ø 130mm.

Spacing can be adjusted from 1 to 5mm.

Soft-touch operation.

Time flow ~3 seconds.

Flow rate set at 0.15 l/sec. at 3 bar, can be adjusted.

Chrome-plated brass body M½".

Suitable for people with reduced mobility.

30-year warranty.

The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).