**TEMPOSOFT 2 time flow urinal valve**

Time flow 3 seconds

For panels, Soft-touch operation

Reference: **777140**

Specification description

Time flow urinal valve for panels:

For standard or siphon action urinals.

For panels or dry wall installation up to 7mm maximum.

Soft-touch operation.

Time flow ~3 seconds.

Flow rate pre-set at 0.15 l/sec. at 3 bar, can be adjusted.

Chrome-plated solid brass body M½".

Suitable for people with reduced mobility.

30-year warranty.