**TEMPOSOFT 2 time flow urinal valve**

Time flow 3 seconds

Angled, Soft-touch operation

Reference: **778800**

Specification description

Exposed time flow urinal valve:

For standard or siphon action urinals.

For wall-mounted exposed installation.

Soft-touch operation.

Time flow ~3 seconds.

Flow rate pre-set at 0.15 l/sec. at 3 bar, can be adjusted.

Chrome-plated solid brass body M½".

Angled for recessed inlet.

Compatible with rain water

Suitable for people with reduced mobility.

30-year warranty.