**TEMPOFLUX 2 direct flush valve**

Direct flush WC valve

Cross wall 140mm, 3L/6L

Reference: **762150**

Specification description

Flush system without cistern: directly connected to pipework.

For walls ≤ 140mm.

3L/6L dual flush can be adjusted to 2L/4L.

Soft-touch operation.

Vacuum breaker.

Integrated stopcock and flow rate / flush volume adjuster.

Solid brass body.

Chrome-plated metal push-button.

In-line inlet M¾".

Outlet connection for PVC tube Ø 26/32mm.

Threaded rod can be cut to size.

Acoustic level complies with European standard EN 12541 class II.

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Compatible with rain water.

Suitable for rimless WC pans without flow rate regulation.

Suitable for people with reduced mobility.

30-year warranty.