**TEMPOFLUX 1 direct flush valve**

Time flow direct flush WC valve

Exposed, built-in stopcock

Reference: **761001**

Specification description

Flush system without cistern: directly connected to pipework.

For wall-mounted exposed installation.

Soft-touch operation.

Time flow ~7 seconds.

Vacuum breaker.

Integrated stopcock and flow/volume rate adjuster.

Chrome-plated solid brass body and push-button.

Angled inlet M¾".

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Suitable for people with reduced mobility.

30-year warranty.