**TEMPOFLUX 1 direct flush kit**

Time flow direct flush WC system

Exposed no stopcock, with tube Ø 24/25mm

Reference: **761025**

Specification description

Flush system without cistern: directly connected to pipework.

For wall-mounted exposed installation.

Soft-touch operation.

Time flow ~7 seconds.

Vacuum breaker.

Chrome-plated solid brass body and push-button.

Angled inlet M¾".

With flush tube Ø 25mm and Ø 24mm (replacements for SCHELL BINE 120000 models).

Upstream supply pipes: minimum Ø 20mm required at all points (including connectors).

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Compatible with rain water.

Suitable for people with reduced mobility.

30-year warranty.