**TEMPOCHASSE direct flush valve**

Time flow direct flush WC valve

Exposed

Reference: **760000**

Specification description

Flush system without cistern: directly connected to pipework.

For wall-mounted exposed installation.

Time flow ~7 seconds.

Vacuum breaker.

Chrome-plated solid brass body and push-button.

Shock-resistant mechanism.

With push-button.

In-line inlet M1¼".

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Compatible with rain water.

30-year warranty.