**Deck-mounted single hole mixer - 45 lpm**

Swivelling over spout L. 200mm H. 190mm

Reference: **G66452**

Specification description

Deck-mounted single hole mixer for professional kitchens.

Mixer for plunge sinks with swivelling, tubular spout H. 190mm L. 200mm.

Star-shaped flow straightener with smooth interior.

Water-free valve heads with control knobs.

Flow rate 45 lpm at 3 bar.

Chrome-plated brass body and spout.

Reinforced fixings via two stainless steel rods.

F3/8" PEX flexibles.

Mixer suitable for intensive use in professional kitchens.

Single hole mixer

30-year warranty.