**Deck-mounted twin hole mixer - 45 lpm**

Swivelling over spout H. 300mm L. 340mm

Can be installed close to the splashback

Reference: **G65603**

Specification description

Deck-mounted twin hole mixer, M1/2" with 100 - 240mm adjustable centres.

Swivelling, tubular spout Ø 22mm H. 340mm L. 300mm with star-shaped flow straightener.

Water-free, guided valve heads with control knobs.

Flow rate 45 lpm at 3 bar.

Spout with smooth interior.

Chrome-plated brass body and spout.

Reinforced fixings.

Can be installed close to the splashback.

30-year warranty.