**Auto-rewind 304 stainless steel hose reel**

With 15m flexible hose and hand spray

Reference: **5675T2**

Specification description

Auto-rewind hose reel with flexible hose L. 15m and guide rollers:

Maximum temperature 50°C.

Flow rate 23 lpm at 3 bar.

Maximum pressure 20 bar, 12 bar with trigger-op hand spray.

Hose reel with 304 Stainless steel base and drum Ø 390mm.

Order separately: an angled stopcock with integrated vacuum breaker to prevent the back flow of polluted water into the mains supply.

Stainless steel hose reel with 30-year warranty.