**Eye wash station**

Wall-mounted - dual spray

Trigger-operated

Reference: **9121**

Specification description

Wall-mounted dual spray eye wash with:

Eye wash spray heads with protective caps in green ABS; will eject automatically when activated.

Press the trigger to operate eye wash spray.

A spring automatically shuts off spray.

Flow rate 9 lpm at 3 bar. Aerators with stainless steel double filters.

Ergonomic grip and trigger in green polypropylene.

Supplied with identification sign for first aid equipment "Eye Wash".

Hook for spray head and flexible hose L. 1.50m.

30-year warranty.