**Hygienic BIOSAFE outlet F22/100**

Pack of 1

Reference: **923022**

Specification description

BIOSAFE hygienic outlet F22/100 for basin mixers and taps.

With no grid or partitions in contact with the water.

Flow rate 5 lpm.

Water cannot stagnate in the internal part, reducing bacterial development.

Made from Hostaform which reduces the build-up of scale.

Chrome-plated brass collar.

Sold individually.

Can only be installed on a mixer/tap with a restricted flow rate to ensure a good flow with no splashing.