**TEMPOMATIC electronic shower kit**

Electronic

Cross wall for 150mm walls, valve, ROUND head

Reference: **452159**

Specification description

Cross wall electronic shower kit:

TEMPOMATIC electronic valve for mixed water supply.

For walls ≤ 155mm.

Power supply by electronic unit with solenoid valve 1/2".

230/12V transformer.

2 operation modes:

- Automatic activation via presence detection.

- Voluntary ON/OFF activation by passing the hand in front of sensor ~10 cm.

Duty flush (~60 seconds every 24 hours after the last use).

Adjustable time flow from 30 to 60 seconds.

Flow rate set at 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

Chrome-plated solid brass.

Wall plate flush to the wall.

Threaded rods can be cut-to-size.

Electronic shower kit suitable for people with reduced mobility.

30-year warranty.