**TEMPOGENOU time flow tap**

Knee-operated

Straight model

Reference: **735400**

Specification description

Knee-operated time flow basin valve:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Reinforced control lever.

Solid brass wall plate with reinforced fixing via 4 stainless steel screws.

Cold or mixed water supply.

Chrome-plated solid brass body M½".

Straight model for in-line.

30-year warranty.