**SECURITHERM EP pressure-balancing shower mixer**

Wall-mounted single control mixer, solid lever

With offset standard connectors

Reference: **2739TEPS**

Specification description

Wall-mounted single control mechanical shower mixer.

Wall-mounted single control mixer with Securitouch thermal insulation to prevent burns.

Ø 40mm pressure-balancing ceramic cartridge with pre-set maximum temperature limiter.

Anti-scalding safety: HW flow is reduced if CW supply fails (and vice versa).

Constant temperature regardless of pressure or flow rate variations in the system.

Body with smooth interior and low water volume.

Flow rate regulated at 9 lpm.

Chrome-plated brass body and solid control lever.

M1/2" shower outlet with integrated non-return valve.

Mixer with offset standard wall connectors, M1/2" M3/4".

Filters and non-return valves on the inlets.

Mechanical mixer with SECURITHERM pressure-balancing ideal for healthcare facilities, retirement homes, hospitals and clinics.

Shower mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.