**Wall-mounted liquid soap dispenser, 0.5 litres**

Liquid soap or hydroalcoholic gel dispenser

Soft-touch, bright polished 304 stainless steel

Reference: **510583**

Specification description

Wall-mounted soap dispenser with soft-touch operation.

Liquid soap or hydroalcoholic gel dispenser.

Vandal-resistant model with lock and standard DELABIE key.

Bacteriostatic 304 stainless steel cover.

One piece hinged cover for easy maintenance and improved hygiene.

Soft-touch push button: suitable for any user, people with reduced mobility, children.

Anti-blocking: one dose per push even if button is held in place.

No waste, non-drip (waterproof) pump dispenser.

Tank with large opening: eases transfer of soap from large containers.

Tank prevents the long-term stagnation of soap.

Window for monitoring soap level.

Bright polished 304 stainless steel.

Stainless steel thickness: 1 mm.

Capacity: 0.5 litres.

Dimensions: 90 x 105 x 185mm.

For vegetable based liquid soap with a maximum viscosity: 3,000 mPa.s.

Compatible with hydroalcoholic gel.

Wall-mounted soap dispenser with 30-year warranty.