**TEMPOMIX time flow shower panel**

Time flow single control

Ø 15mm top inlet, handset, aluminium

Reference: **79035015**

Specification description

Time flow shower panel with handset:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Top inlet via in-line stopcocks and conical Ø 15mm inlets.

TEMPOMIX mixer with adjustable maximum temperature limiter.

Soft-touch operation.

Time flow ~30 seconds.

Sliding handset on chrome-plated rail with flexible hose.

Concealed fixings.

Filters and non-return valves.

30-year warranty.