**SECURITHERM thermostatic basin mixer**

Single hole thermostatic sequential mixer, H. 95mm L. 120mm

Stopcocks and Hygiene lever L. 146mm, Ø 15mm

Reference: **H960015**

Specification description

Deck-mounted SECURITHERM thermostatic basin mixer.

Thermostatic sequential mixer: opens and closes with cold water.

No risk of cross flow between hot and cold water.

No non-return valves on the inlets.

Anti-scalding failsafe: shut-offs automatically if cold or hot water supply fails.

Securitouch thermal insulation prevents burns.

Single hole mixer with curved spout H. 95mm L. 120mm, equipped with a hygienic flow straightener with no impurity retention and will withstand thermal shocks.

Scale-resistant sequential thermostatic cartridge for single lever control of the flow rate and temperature.

Temperature control from cold water up to 40°C with temperature limiter set at 40°C.

Thermal or chemical shocks are possible.

Body and spout with smooth interiors and low water volume.

Flow rate limited to 5 lpm at 3 bar.

No manual contact thanks to Hygiene control lever L. 146mm.

No pop-up waste.

PEX flexibles F3/8" supplied with stopcocks in chrome-plated brass, filters and Ø 15mm compression fittings.

Fixing reinforced by 2 stainless steel rods.

Mixer ideal for healthcare facilities, nursing homes, hospitals and clinics.

Mixer Suitable for people with reduced mobility.

Mixer with 30-year warranty.

Also available with copper tails.