**BINOPTIC MIX electronic mixer**

Battery operated, Ø 15mm conical inlets

Standard control, Spout with smooth interior

Reference: **478MCH15**

Specification description

Deck-mounted electronic basin mixer:

Independent IP65 electronic control unit.

123 6V Lithium battery.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Active, infrared movement detection, sensor at the end of the spout optimises detection.

Chrome-plated solid brass body.

PEX flexibles with filters, solenoid valves and Ø 15mm conical inlets.

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Spout with a smooth interior and low volume of water (limits bacterial niches).

Side temperature control with adjustable maximum temperature limiter.

30-year warranty.