**F3/8" rotating PEX flexible hoses**

L. 465mm

2 per pack

Reference: **FLEXPEX6**

Specification description

Rotating flexible hoses F3/8” made from braided stainless steel with Ø 6mm PEX core for mixer 2620.

Rotating unions to simplify installation (non-twist).

Withstand thermal and chlorine shocks: maximum temperature 90°C (recommended 65°C).

Maximum pressure: 10 bar.

Can be removed.

2 per pack.