**TEMPOMATIC tap with BIOCLIP removable spout**

Wall-mounted electronic tap with mains supply

Mains supply

Reference: **20804T215**

Specification description

Wall-mounted electronic basin tap for installation on panels.

Electronic tap with removable BIOCLIP spout.

Infrared tap supplied with 2 removable stainless steel spouts L. 77mm.

Separate IP65 electronic control unit.

230/12V mains supply with transformer.

Base and spout with smooth interiors (reduces bacterial development).

Adjustable duty flush (pre-set at ~60 seconds every 24 hours after last use).

Flow rate limited to 4 lpm at 3 bar.

Shock-resistant infrared presence detection sensor.

Separate sensor for mounting on panels.

M3/8" solenoid valve with filter and Ø 15mm conical inlets.

Ø 60mm chrome-plated brass base.

Anti-blocking security.

Recommended installation height: 110 - 200mm above the basin surface.

Electronic tap ideal for healthcare facilities, retirement and care home, hospitals and clinics.

Electronic tap suitable for people with reduced mobility.

30-year warranty.

Two shut-off options:

- standard mode: timed flow with automatic shut-off.

- ON/OFF mode: user shuts off flow voluntarily or automatic shut-off after 30 minutes of flow.

Thermal shocks are possible.

Mount the sensor to the side of the tap in the ON/OFF mode.