**Floor-standing ILHA JR drinking fountain**

Polished satin 304 stainless steel

With built-in tap - H. 800mm

Reference: **180110**

Specification description

Floor-standing drinking fountain.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 1.5mm.

Height: 800mm for children.

Supplied with bubbler tap: chrome-plated, instant shut-offand adjustable flow rate, inlet M⅜".

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Recessed vertical water outlet. Waste outlet 1¼".

Weight: 9kg.

30-year warranty.

[Formerly ref: 0810110000]