**PMR XS TC wall-mounted washbasin**

Polished satin 304 stainless steel - For people with reduced mobility

With no tap hole

Reference: **160250**

Specification description

Wall-mounted washbasin, cross wall installation for service ducts.

Basin internal diameter: 310mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Vandal-resistant: shrouded basin, concealed waste outlet.

200mm threaded rod can be cut to size (other lengths available on request).

Recessed horizontal waste outlet Ø 32mm.

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 4.5kg.

[Formerly ref: 3416250000]