**DUO S TC L washbasin**

Polished satin 304 stainless steel - Wall-mounted with concealed waste

With no tap hole

Reference: **160370**

Specification description

Wall-mounted washbasin with through-the-wall installation for service ducts.

Integrated countertop.

Left hand basin.

Basin internal diameter: 310mm. Polished satin finish. Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm

Rounded edges prevent injury.

Vandal-resistant: shrouded basin, concealed waste outlet.

200mm threaded rod can be cut to size (other lengths are available on request).

Recessed horizontal waste outlet Ø 1".

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Without overflow. Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 8.5kg.

[Formerly ref: 0216370000]