**SECURITHERM time flow shower panel**

Time flow thermostatic and mechanical dual control

Top inlet, fixed and handheld showerhead, st steel

Reference: **792324**

Specification description

Thermostatic dual control shower panel:

Large satin stainless steel shower panel for wall mounted, exposed installation.

With top inlet via in-line stopcocks, M½".

SECURITHERM thermostatic shower mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Chrome-plated, tamperproof, scale-resistant, fixed, ROUND shower head with automatic flow rate regulation at 6 lpm at 3 bar.

Handset with removable flexible via push-fit rapid STOP connector, wall support supplied.

~30 second time flow valve with soft-touch operation to control fixed ROUND shower head

1/4 turn non-time flow valve to control handset with flexible hose.

Thermal shocks are possible.

Concealed fixings.

Filters and non-return valves.

Shower panel suitable for people with reduced mobility.

30-year warranty.