**Splash guard shower curtain rail**

Lift-up

Polished satin 304 stainless steel

Reference: **510159S**

Specification description

Lift-up splash guard shower curtain rail.

Allows side access in the raised position for people with reduced mobility.

Preserves the patient's privacy in the lowered position.

Allows a carer to assist with bathing a patient while protecting them from splashes.

Dimensions: 900 x 230 x 105mm, Ø 32mm.

Retained in upright position.

Slowed down descent.

UltraSatin polished satin bacteriostatic 304 stainless steel lift-up curtain rail.

Fixings concealed by a 4mm thick 304 stainless steel cover plate.

Supplied with stainless steel screws for concrete walls.

30-year warranty.