**Pressure-balancing mixer set and column with retracting hand spray**

EP sink mixer with retractable hand spray

Mixer with sculptured lever

Reference: **2599EP**

Specification description

Sink mixer with hand spray and column with retractable hand spray.

Single hole mixer with pressure-balancing and column suitable for baby baths.

Swivelling column H. 200mm L. 220mm.

With retracting hand spray with two jet options (flow straightener/rain effect).

Ø 35mm pressure-balancing ceramic cartridge with pre-set maximum temperature limiter.

Total anti-scalding safety: HW flow rate is reduced if CW supply fails (and vice versa).

Stable temperature regardless of variations in pressure and flow rate in the system.

Securitouch thermal insulation prevents burns.

Single hole mixer body and column with smooth interior.

Flow rate limited to 7 lpm at 3 bar.

Sculptured control lever.

BIOSAFE flexible hose reduces the spread of germs: transparent polyurethane flexible hose ensures replacement if biofilm is present, smooth interior and exterior.

Flexible hose with narrow diameter (internal Ø 6mm): low water volume.

Specific counterweight.

Body in chrome-plated brass

F⅜" PEX flexibles

SECURITHERM pressure-balancing mechanical mixer with hand spray, ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

single hole mixer suitable for people with reduced mobility.

Single control mixer with 30-year warranty.