**Wall-mounted FRAJU PMR washbasin**

Polished satin 304 stainless steel

With Ø 35mm centre tap hole

Reference: **121440**

Specification description

Wall-mounted washbasin, 620x505mm.

Suitable model for people with reduced mobility.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm for the bowl and 1.5mm for surround.

Rounded edges prevent injury.

With Ø 35mm central tap hole.

Supplied with 1¼" waste.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 5kg.

30-year warranty.