**Wall-mounted CANAL wash trough**

Polished satin 304 stainless steel - L. 1200mm

With 2 Ø 22mm tap holes

Reference: **121250**

Specification description

Wall-mounted wash trough for wall-mounting, for 2 services - 1,200mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 0.8mm for the bowl, 1.5mm for surround and fixing brackets.

Easy to install: no joint concealers to install, lightweight trough.

Drainage on the right.

With 2 tap holes Ø 22mm.

Supplied with M1"1/4 waste. Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14296.

Weight: 7.6kg.

30-year warranty.

Option to add a bacteriostatic 304 stainless steel splashback (ref. 100250).

[Formerly ref: 0211250018]