**MONOBLOCO 700 PMR WC pan with cistern**

Polished satin 304 stainless steel

Reference: **110790**

Specification description

Floor-standing WC pan with dual flush cistern 3L/6L, 370 x 895 x 700mm.

700mm elongated pan for better comfort for people with reduced mobility.

Bacteriostatic 304 stainless steel. Polished satin finish.

Stainless steel thickness: 1.5mm.

One-piece pressed WC bowl, seam-free for better hygiene.

WC bowl surface is polished with rounded edges for easy cleaning.

Concealed perimetral flushing rim. Water supply can be recessed from below or exposed from the side (right/left).

Recessed horizontal or vertical waste outlet. Supplied with PVC pipe.

Pre-drilled holes for fixing the toilet seat. Supplied with stainless steel blanking caps when installed without toilet seat lid.

Quick to install: 2 access panels with theft prevention TORX security screws.

CE marked. Complies with European standard EN 997 for 4L flush.

Weight: 22kg.

30-year warranty.