**COMMISSARIAT stainless steel washbasin for recessed installation**

Polished satin 304 stainless steel

Reference: **160330**

Specification description

Wall-mounted washbasin, cross wall installation for service ducts.

Interior basin dimensions: 290 x 290 x 350mm.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 2mm.

Rounded edges prevent injury.

Suitable for prisons, police stations, etc.

Vandal-resistant: water inlet and outlet cannot be accessed by user.

Supplied without water controls. We recommend electronic control: ref. 447100.

Weight: 12.5kg.