**Wall-mounted SXS mechanical hand washbasin**

Polished satin 304 stainless steel - Knee-operated - with upstand

Without tap

Reference: **181320**

Specification description

Wall-mounted hand washbasin.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 0.8mm.

Rounded edges prevent injury.

With splashback.

Model without tap.

Complete model, with tap and premixer is available (ref. 182320).

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 4.3kg.

30-year warranty.