**SECURITHERM time flow shower panel**

Time flow thermostatic, comfort 10 lpm

Concealed inlet, fixed sh. head, st. steel

Reference: **792313CF**

Specification description

Thermostatic time flow shower panel:

Large model satin stainless steel shower panel for wall mounted, exposed installation.

Concealed inlet via flexibles M½".

SECURITHERM thermostatic shower mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold or hot water supply fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Soft-touch operation.

Chrome-plated, tamperproof, scale-resistant, fixed, ROUND shower head with automatic flow rate regulation.

Time flow ~30 seconds.

Flow rate 10 lpm at 3 bar.

M½" stopcocks.

Concealed fixings.

Filters and non-return valves.

Shower panel suitable for people with reduced mobility.

30-year warranty.