**SECURITHERM dual control shower panel**

Mechanical thermostatic dual control, comfort 10 lpm

Top inlet, fixed shower head + handset, st. steel

Reference: **792344CF**

Specification description

Dual control thermostatic shower panel:

Large model satin stainless steel shower panel for wall mounted, exposed installation.

Top inlet via inline stopcocks M½".

SECURITHERM thermostatic shower mixer.

Adjustable temperature control from cold water up to 38°C with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if cold or hot water supply fails.

Chrome-plated, tamperproof, scale-resistant, fix, ROUND shower head with automatic flow rate regulation at 10 lpm at 3 bar.

Handset with removable flexible via rapid push-fit STOP connector, wall support supplied.

2 non-time flow valves control fixed ROUND shower head and handset with flexible hose.

Thermal shocks are possible.

Concealed fixings.

Filters and non-return valves.

Shower panel suitable for people with reduced mobility.

30-year warranty.