**ROUND shower head**

Scale-resistant, comfort 10 lpm

Recessed

Reference: **709000CF**

Specification description

Fixed shower head:

Recessed installation.

Flow rate 10 lpm at 3 bar.

Automatic flow rate regulation.

Scale-resistant and ligature-resistant adjustable nozzle.

Chrome-plated solid brass.

Fixed with hidden blocking screw.

Systematically drains after use (no water or impurity retention).

Inlet M½".

30-year warranty.