**Connection kit for disabled WCs**

For TEMPOFIX 3 frame system

Reference: **578PMR**

Specification description

Extended supply tube Ø 32mm, L. 580mm.

Ø 55mm connection washer.

30-year warranty.