**TEMPOMIX 3 time flow mixer**

Soft-touch operation

Single control, wall-mounted, Kit 2/2 L. 190mm

Reference: **794055**

Specification description

Wall-mounted single control time flow basin mixer, Kit 2/2:

Soft-touch operation.

Temperature control and operation via the push-button.

Time flow pre-set at ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Tamperproof, scale-resistant flow straightener.

Chrome-plated solid brass body L. 190mm.

Wall-mounted M½".

Top or bottom supply.

Recessed inlets.

Filters and non-return valves.

Adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.

To order with inlet reference 794012.