**BOB HD washbasin**

Polished satin 304 stainless steel - Wall-mounted - Concealed drainage

Without tap hole

Reference: **164130**

Specification description

Wall-mounted hand washbasin.

Basin internal diameter: 310mm.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Vandal-resistant: shrouded basin, concealed trap, reinforced mounting frame.

Quick and easy to install from the front thanks to a stainless steel mounting frame.

Supplied with 1½" waste and trap.

Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 5.5 kg.