**Basic two-wall shower grab bar with sliding vertical bar, white**

White powder-coated stainless steel

Ø 32mm

Reference: **35481W**

Specification description

Basic two-wall grab bar with sliding vertical bar, for people with reduced mobility.

White powder-coated stainless steel.

Upright position can be adjusted during installation: can be moved to the left or the right.

Concealed fixings, secured to wall by a 3-hole plate.

Dimensions: 1,150 x 750 x 750mm, Ø 32mm.

30-year warranty.

CE marked.