**DELTA TC wall-hung urinal**

Polished satin 304 stainless steel - Rear inlet

Reference: **160770**

Specification description

Wall-hung individual rimless urinal, cross wall installation for service ducts.

Bacteriostatic 304 stainless steel. Stainless steel thickness: 1.2mm.

Rear (recessed) inlet.

Vandal-resistant: recessed waste outlet, concealed trap.

200mm threaded rod can be cut to size (other lengths available on request).

Supplied with fixing elements.

CE marked. Complies with European standard EN 13407 for 2L flush.

Weight: 8kg.