**Mechanical sink mixer**

Wall-mounted mixer, fixed L. 150mm spout, Hygiene lever L. 150mm

With STOP/CHECK connectors

Reference: **2447LUK**

Specification description

Wall-mounted mechanical basin mixer, 200mm centres.

Flat fixed under spout L. 150mm with hygienic flow straightener suitable for fitting a BIOFIL terminal filter.

Securitouch thermal insulation prevents burns.

Ø 40mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume (reduce niches where bacteria can develop).

Flow rate regulated at 5 lpm.

Chrome-plated brass body.

Hygiene control lever L. 150mm.

Supplied with in-line STOP/CHECK connectors M1/2" M3/4" ideal for hospitals.

30-year warranty.