**TEMPOMATIC 4 electronic tap**

Integrated batteries

For walls L. 190mm, integrated electronics

Reference: **443516**

Specification description

Wall-mounted electronic basin tap:

Lithium 123 6V batteries integrated.

Reduced-stagnation solenoid valve and electronic unit integrated into the body of the tap.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Sensor at the end of the spout optimises presence detection.

Chrome-plated stainless steel body, L. 190mm.

Cap fixed in place by 2 concealed screws.

Stopcock.

For cross wall installation.

Anti-blocking security.

Suitable for people with reduced mobility.

30-year warranty.