**Flush tube**

For WC pan with TEMPOMATIC, TEMPOFLUX or TEMPOCHASSE

PVC and HDPE

Reference: **769500**

Specification description

Cross wall/recessed flush tube for WC pans:

For TEMPOMATIC, TEMPOFLUX 1, TEMPOFLUX 2, TEMPOFLUX 3 and TEMPOCHASSE.

PVC tube, HDPE pipe.

For recessed or cross wall installation on walls ≥ 60mm.

Ø 26/32mm pipe with Ø 55 mm connection washer.

W. 670mm, H. 703-783mm.

30-year warranty.