**TEMPOSTOP urinal valve**

Time flow 7 seconds

Angled ½"

Reference: **778007**

Specification description

Exposed time flow urinal valve:

For standard, siphon action or stall urinals.

For wall-mounted installation.

Time flow ~7 seconds.

Flow rate pre-set at 0.15 L/sec. at 3 bar, can be adjusted.

Compatible with rain water.

Chrome-plated solid brass body M½".

Wall plate.

Angled for recessed inlets.

30-year warranty.