**TEMPOSTOP urinal valve**

Time flow 3 seconds

Recessed, with stainless steel wall plate

Reference: **777930**

Specification description

Recessed time flow urinal valve.

For standard or siphon action urinals.

For recessed installation.

Recessing depth can be adjusted from 20 to 35mm.

Stainless steel wall plate Ø 130mm.

Time flow ~3 seconds.

Flow rate pre-set at 0.15 l/sec. at 3 bar, can be adjusted.

Solid brass body M½".

30-year warranty.

This model does not have a waterproof recessing box. The installer must ensure that the recessing area is waterproof and any leaks or condensates can drain away (see installation guide).